The CFontz Driver
This section talks about using LCDproc with the serial LCD displays of the CFA632 and CFA634 series by CrystalFontz, Inc.

Configuration in LCDd.conf

[CFontz]
Device = DEVICE 	 Select the serial output device to use. If not given, default is /dev/lcd.
Size = 	 Set the LCD's dimensions in terms of characters per line and lines. If not given, it defaults to 20x4.
Contrast = CONTRAST 	 Set the initial contrast. Legal values for CONTRAST are in the range between 0 and 1000. If not given, it defaults to 560.
Brightness = BRIGHTNESS 	 Set the initial brightness. Legal values for BRIGHTNESS range from 0 to 1000. If not given, it defaults to 1000.
OffBrightness = BRIGHTNESS 	 Set the initial off-brightness. This value is used when the display is normally switched off in case LCDd is inactive. Legal values BRIGHTNESS are in the range from 0 to 1000. The default is 0.
Speed = { 1200 | 2400 | 9600 | 19200 | 115200 } 	 Set the the baud rate to use when communicating with the LCD. It defaults to 9600 if not specified.
NewFirmware = 	 Set the firmware version (New means >= 2.0) [default: no; legal: yes, no].
Reboot = 	 Reinitialize the LCD's BIOS [default: no; legal: yes, no] normally you shouldn't need this.