The NoritakeVFD Driver
This section talks about using LCDproc with text mode VFD displays from Noritake Itron.

Configuration in LCDd.conf

[NoritakeVFD]
Device = DEVICE 	 Port where the VFD is. Usual values are /dev/ttyS0 and /dev/ttyS1 Default: /dev/lcd
Size = 	 Specifies the size of the LCD. Default: 20x4
Brightness = BRIGHTNESS 	 Set the initial brightness [default: 1000; legal: 0 - 1000]
OffBrightness = BRIGHTNESS 	 Set the initial off-brightness [default: 0; legal: 0 - 1000] This value is used when the display is normally switched off in case LCDd is inactive
Speed = { 1200 | 2400 | 9600 | 19200 | 115200 } 	 Set the the baud rate to use when communicating with the VFD. If not specified, it defaults to 9600.
Parity = { 0 | 1 | 2 } 	 Set the parity for communication with the device to even parity (2), odd parity (1) or no parity (0). If not given, it defaults to 0.
Reboot = 	 Reinitialize the VFD [default: no; legal: yes, no]