The SureElec Driver
Driver for the LCD modules (actually the controller board) available from the 'SURE electronics' shop ().
These devices are PIC based controlled, using a serial communication protocol with the host. The actual connection to host is done through USB through a serial-to-USB converter (CP2102 USB to UART Bridge) integrated on the board.

Configuration in LCDd.conf

[SureElec]
Device = DEVICE 	 Name of the device the display appears as. By default first USB serial device /dev/ttyUSB0 is used.
Edition = EDITION 	 Edition level of the device (can be 1, 2 or 3). The default is 2.
Size = 	 Set the display size in characters. This is required for edition 1 devices. For edition 2 & 3 devices this value, if defined, overrides the size read directly from the device.
Contrast = CONTRAST 	 Select the display's contrast, 480 is the default. Permissible values are in the range of 0-1000.
Brightness = BRIGHTNESS 	 Select the display's brightness, 480 is the default. Permissible values are in the range of 0-1000.
OffBrightness = OFFBRIGHTNESS 	 Select the display's when the display is normally switched off in case LCDd is inactive, 100 is the default. Permissible values are in the range of 0-1000.