The ea65 driver
This section describes the ea65 driver which works with the front panel VFD display on the AOpen XC Cube-AV EA65 media barebone.

EA65 front panel VFD
The AOpen XC Cube-AV is a barebone designed for using as a media center. It comes with a front panel display which is capable of displaying one line of 9 characters.
The display is internally connected to the serial port (/dev/ttyS1) with a fixed rate of 9600 baud.
The display uses 13 segments per character. That's why the driver provides no custom characters like the ones for dot matrix displays do.
The front panel furthermore has 9 keys which are illuminated by blue LEDs. The LEDs can be controlled with the backlight functions. The keys are not supported by this driver. The red LED (RECORD) can be controlled with the output command of LCDd.

Configuration in LCDd.conf

[ea65]
Brightness = BRIGHTNESS 	 Set the brightness for the front LEDs if backlight is switched on. Legal values for BRIGHTNESS are in the range between 0 and 1000. Values under 300 set the LEDs off. Values between 300 and 700 turn on the LEDs with half brightness. Values above 700 turn on the LEDs with full brightness. If not given, it defaults to 500.
OffBrightness = OFFBRIGHTNESS 	 Set the brightness for the front LEDs if backlight is switched off. Legal values for OFFBRIGHTNESS are in the range between 0 and 1000. Values under 300 set the LEDs off. Values between 300 and 700 turn on the LEDs with half brightness. Values above 700 turn on the LEDs with full brightness. If not given, it defaults to 0.