The glk Driver
This section talks about using LCDproc with LCD displays that use the Matrix Orbital GLK and GLC chipset.

Supported devices
Currently the drivers supports the following devices:
GLC12232 (20x4)
GLC12864 (20x8)
GLC128128 (20x16)
GLC24064 (40x8)
GLK12232-25 (20x4)
GLK12232-25-SM (20x4)
GLK12864-25 (20x8)
GLK128128-25 (20x16)
GLK24064-25 (40x8)
Modules not in the list above are not recognized and the driver will not load if it encounteres an unrecognized display.

Configuration in LCDd.conf

[glk]
Device = DEVICE 	 select the serial device to use [default: /dev/lcd]
Contrast = CONTRAST 	 Set the initial contrast. Legal values for CONTRAST are 0 - 1000. If not given, it defaults to 560.
Speed = { 9600 | 19200 | 38400 } 	 Set the the baud rate for communication with the LCD. The default is 19200.