The i2500vfd Driver
This section talks about using LCDproc with an Intra2net Intranator 2500 VFD display. The displays are part of a custom high grade steel chassis and not sold separately. More information can be found here: Intra2net AG
It connects to USB using a FTDI FT245BM chip and therefore needs libftdi as requirement. libftdi can be found here: libftdi

Features
The display features a 140x32 pixel Noritake VFD tube which gets driven by an Atmel ATmega128 processor and used as a 23x4 character display with a 6x8 pixel font. It features B/W colors and two additional adjustable grayscale colors. It does hardware double buffering with up to 27 FPS and shows an animated boot logo until data is received from USB.

Options
There are currently no options for this driver.