The icp_a106 Driver
This section talks about using LCDproc with the ICP Peripheral Communication Protocol used by A125 and A106 LCD displays
Both LCD and alarm functions are accessed via one serial port, using separate commands. Unfortunately, the device runs at slow 1200bps and the LCD does not allow user-defined characters, so the bargraphs do not look very nice. The A125 does include two buttons marked ENTER and SELECT. Short press of ENTER: ENTER Long press of ENTER: ESC Short press of SELECT: DOWN Long press of SELECT: UP

Configuration in LCDd.conf

[icp_a106]
Device = DEVICE 	 Sets the device to use. Defaults to /dev/lcd.
Size = SIZE 	 Sets the display resolution to use. Defaults to 20x2