The Joystick Input Driver
This section covers the joystick input driver for LCDd.

Configuration in LCDd.conf

[joy]
Device = DEVICE 	 Select the input device to use [default: /dev/js0]
Map_AxisNUMneg = KEY 	 Map_AxisNUMpos = KEY 	 Set the axis map.
NUM is an integer starting with 1 that represents each axis with the affixes neg and pos determining the direction. The exact numbering of the axes depends on the hardware used.
KEY can be one of the keys that LCDd recognizes (Left, Right, Up, Down, Enter or Escape) or any other string that a client can parse.
Map_ButtonNUM = KEY 	 Set the button map.
NUM is an integer starting with 1 that represents each button. The exact numbering of the buttons depends on the hardware used.
KEY can be one of the keys that LCDd recognizes (Left, Right, Up, Down, Enter or Escape) or any other string that a client can parse.