The mtc_s16209x Driver
This section talks about using LCDproc with LCD displays that use the mtc_s16209x chipset.

Configuration in LCDd.conf

[mtc_s16209x]
Device = DEVICE 	 Select the output device to use [default: /dev/lcd]
Brightness = BRIGHTNESS 	 Set the initial brightness [default: 255; legal: 0 - 255]
Reboot = 	 Reinitialize the LCD's BIOS [default: no; legal: yes, no]