The MX5000 Driver
This section talks about using LCDproc with LCD displays on Logitech MX5000 keyboards.

Features
This drivers uses the library from mx5000tools.

Configuration in LCDd.conf

[mx5000]
Device = DEVICE 	 Select the output device to use [default: /dev/hiddev0]
WaitAfterRefresh = MS 	 Set the time (in ms) to wait after each screen sent to the keyboard. Default is 1000ms.