The stv5730 Driver
This section talks about using LCDproc with LCD displays that use the stv5730 chipset.

Configuration in LCDd.conf

[stv5730]
Port = PORT 	 Specify the address of the parallel port the LCD is connected to. Common values for PORT are 0x278, 0x378 and 0x3BC. If not given, it defaults to 0x378.