The tyan Driver
This section talks about using LCDproc with LCD modules used in Tyan GS10 and GS12 barebones.

Features
The LCD modules used on the front side of the Tyan GS10 and GS12 series barebones consist of an LCD display by Winstar Display Co. LTD that is 16 characters wide and 2 lines high. To the right of the display there is a 6 button keypad: 4 array buttons and two buttons labeled C and S.
For more information see the LCD pack from the Tyan support page. Besides a useless old version of LCDproc it contains some documentation about the panel itself including a PDF specification of the LCD display by its manufacturer.

Configuration in LCDd.conf

[tyan]
Device = DEVICE 	 Select the output device to use [default: /dev/lcd]
Speed = { 4800 | 9600 } 	 Set the the baud rate communication with the LCD. If not given, the default is 9600.
Size = 	 set display size [default: 16x2]