The yard2 driver

General
The yard2 driver handles the yard2 LCD device. The driver functionality is currently limited to character LCD.
This driver writes via socket to yard2srvd deamon.
The yard2 driver assumes the character encoding ISO 8859-1.

Configuration
The only configuration parameter is Size. All other settings are done in yard2srvd daemon.