The MD8800 Driver
This section talks about using LCDproc with VFD displays in Medion MD8800 PCs.

Features
You may find more information about the LCD on Martin Moeller's homepage.

Configuration in LCDd.conf

[MD8800]
Device = DEVICE 	 device to use [default: /dev/ttyS1]
Size = 	 display size [default: 16x2]
Brightness = BRIGHTNESS 	 Set the initial brightness [default: 1000; legal: 0 - 1000]
OffBrightness = BRIGHTNESS 	 Set the initial off-brightness [default: 0; legal: 0 - 1000] This value is used when the display is normally switched off in case LCDd is inactive