The lcdm001 Driver
This section talks about using LCDproc with serial LCD displays from kernel concepts.

Configuration in LCDd.conf

[lcdm001]
Device = DEVICE 	 Default: /dev/lcd
PauseKey = KEY 	 BackKey = KEY 	 ForwardKey = KEY 	 MainMenuKey = KEY 	 keypad settings
key name	function (normal context)	function (menu context)
PauseKey	Pause/Continue	Enter/select
BackKey	Back(Go to previous screen)	Up/Left
ForwardKey	Forward(Go to next screen)	Down/Right
MainMenuKey	Open main menu	Exit/Cancel
You can rearrange the settings here.
If your device is broken, have a look at server/drivers/lcdm001.h